(export (version D)
  (design
    (source /home/penko/SVN_Checkout/MOD-LCD2.8RTP/Hardware/trunk/BRD/MOD-LCD2.8RTP_Rev_C.sch)
    (date "30.09.2022 (пт) 15:24:50 EEST")
    (tool "Eeschema 5.1.6-c6e7f7d~87~ubuntu18.04.1")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title MOD-LCD2.8RTP)
        (company "Olimex LTD")
        (rev C)
        (date 2022-09-30)
        (source MOD-LCD2.8RTP_Rev_C.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref C1)
      (value 1uF/10V/10%/X5R/C0603)
      (footprint OLIMEX_RLC-FP:C_0603_5MIL_DWS)
      (libsource (lib OLIMEX_RCL) (part C_Small) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 58EDFC31))
    (comp (ref R2)
      (value 22R/R0603)
      (footprint OLIMEX_RLC-FP:R_0603_5MIL_DWS)
      (libsource (lib OLIMEX_RCL) (part R_Small) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 58EE1092))
    (comp (ref R3)
      (value 22R/R0603)
      (footprint OLIMEX_RLC-FP:R_0603_5MIL_DWS)
      (libsource (lib OLIMEX_RCL) (part R_Small) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 58EE1098))
    (comp (ref R4)
      (value 22R/R0603)
      (footprint OLIMEX_RLC-FP:R_0603_5MIL_DWS)
      (libsource (lib OLIMEX_RCL) (part R_Small) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 58EE109E))
    (comp (ref R6)
      (value 4.7k/R0603)
      (footprint OLIMEX_RLC-FP:R_0603_5MIL_DWS)
      (libsource (lib OLIMEX_RCL) (part R_Small) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 58EE316C))
    (comp (ref R5)
      (value 100k/R0603)
      (footprint OLIMEX_RLC-FP:R_0603_5MIL_DWS)
      (libsource (lib OLIMEX_RCL) (part R_Small) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 58EE3383))
    (comp (ref U1)
      (value "NA(AR1021T-I/SS(SSOP-20))")
      (footprint OLIMEX_IC-FP:SSOP-20W)
      (libsource (lib OLIMEX_IC) (part "AR1021T-I_SS(SSOP-20)") (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AD398A8))
    (comp (ref C2)
      (value "NA(1uF/10V/10%/X5R/C0603)")
      (footprint OLIMEX_RLC-FP:C_0603_5MIL_DWS)
      (libsource (lib OLIMEX_RCL) (part C_Small) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5ADFF248))
    (comp (ref R7)
      (value "NA(20k/R0603)")
      (footprint OLIMEX_RLC-FP:R_0603_5MIL_DWS)
      (libsource (lib OLIMEX_RCL) (part R_Small) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AE1C324))
    (comp (ref R8)
      (value 4.7k/R0603)
      (footprint OLIMEX_RLC-FP:R_0603_5MIL_DWS)
      (libsource (lib OLIMEX_RCL) (part R_Small) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AE5CEF3))
    (comp (ref R9)
      (value 4.7k/R0603)
      (footprint OLIMEX_RLC-FP:R_0603_5MIL_DWS)
      (libsource (lib OLIMEX_RCL) (part R_Small) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AE5CF6E))
    (comp (ref R10)
      (value 20k/R0603)
      (footprint OLIMEX_RLC-FP:R_0603_5MIL_DWS)
      (libsource (lib OLIMEX_RCL) (part R_Small) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AD0BFB4))
    (comp (ref SJ1)
      (value "Closed(1-2)")
      (footprint OLIMEX_Jumpers-FP:SJ_2_SMALL_12_TIED)
      (libsource (lib OLIMEX_Jumpers) (part "SJ2W_Closed(1-2)") (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AE9F495))
    (comp (ref SJ5)
      (value "Closed(1-2)")
      (footprint OLIMEX_Jumpers-FP:SJ_2_SMALL_12_TIED)
      (libsource (lib OLIMEX_Jumpers) (part "SJ2W_Closed(1-2)") (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AEBAC81))
    (comp (ref SJ4)
      (value "Closed(1-2)")
      (footprint OLIMEX_Jumpers-FP:SJ_2_SMALL_12_TIED)
      (libsource (lib OLIMEX_Jumpers) (part "SJ2W_Closed(1-2)") (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AEBADEA))
    (comp (ref SJ2)
      (value "Closed(1-2)")
      (footprint OLIMEX_Jumpers-FP:SJ_2_SMALL_12_TIED)
      (libsource (lib OLIMEX_Jumpers) (part "SJ2W_Closed(1-2)") (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AF620ED))
    (comp (ref SJ3)
      (value open)
      (footprint OLIMEX_Jumpers-FP:SJ)
      (libsource (lib OLIMEX_Jumpers) (part SJ) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B28D043))
    (comp (ref LCD1)
      (value "(CXT280H02H34-200P50R)+(FPV-WZB21-50-LF)")
      (footprint OLIMEX_Connectors-FP:FPV-WZB21-50-LF)
      (libsource (lib OLIMEX_Connectors) (part CONN_01X50) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 58EDF962))
    (comp (ref R1)
      (value 22R/R0603)
      (footprint OLIMEX_RLC-FP:R_0603_5MIL_DWS)
      (libsource (lib OLIMEX_RCL) (part R_Small) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 58EE108C))
    (comp (ref C4)
      (value 1uF/10V/10%/X5R/C0603)
      (footprint OLIMEX_RLC-FP:C_0603_5MIL_DWS)
      (libsource (lib OLIMEX_RCL) (part C_Small) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AD0C088))
    (comp (ref U2)
      (value "NS2009(MSOP-10)")
      (footprint OLIMEX_IC-FP:MSOP-10_Pitch-0.5mm_3.00x3.00x1.00mm)
      (libsource (lib OLIMEX_IC) (part "NS2009(MSOP-10)") (description "4-Wire Touch Screen Controller with I2C Interface"))
      (sheetpath (names /) (tstamps /))
      (tstamp 63359B24))
    (comp (ref UEXT1)
      (value "(P-B-V-10-LF)+(CABLE-IDC10-15CM)")
      (footprint OLIMEX_Connectors-FP:UEXTM-SMD)
      (libsource (lib OLIMEX_Connectors) (part BH10S) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 58EE23B5))
    (comp (ref C5)
      (value 100nF/Y5V/50VDC/20%/C0603)
      (footprint OLIMEX_RLC-FP:C_0603_5MIL_DWS)
      (libsource (lib OLIMEX_RCL) (part C_Small) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 63673CF4))
    (comp (ref C6)
      (value 1uF/10V/10%/X5R/C0603)
      (footprint OLIMEX_RLC-FP:C_0603_5MIL_DWS)
      (libsource (lib OLIMEX_RCL) (part C_Small) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 6370DB56))
    (comp (ref C3)
      (value 1uF/10V/10%/X5R/C0603)
      (footprint OLIMEX_RLC-FP:C_0603_5MIL_DWS)
      (libsource (lib OLIMEX_RCL) (part C_Small) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 58EE51CA))
    (comp (ref mUEXT1)
      (value FPV-WZA21-12-LF)
      (footprint OLIMEX_Connectors-FP:FPV-WZB21-12-LF)
      (libsource (lib OLIMEX_Connectors) (part CONN_01X12) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 6336899C))
    (comp (ref FET1)
      (value WPM2015-3/TR)
      (footprint OLIMEX_Transistors-FP:SOT23)
      (libsource (lib OLIMEX_Transistors) (part P-MOS+DIOD) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 639EDAB1)))
  (libparts
    (libpart (lib OLIMEX_Connectors) (part BH10S)
      (fields
        (field (name Reference) CON)
        (field (name Value) BH10S))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num 3) (name 3) (type passive))
        (pin (num 4) (name 4) (type passive))
        (pin (num 5) (name 5) (type passive))
        (pin (num 6) (name 6) (type passive))
        (pin (num 7) (name 7) (type passive))
        (pin (num 8) (name 8) (type passive))
        (pin (num 9) (name 9) (type passive))
        (pin (num 10) (name 10) (type passive))))
    (libpart (lib OLIMEX_Connectors) (part CONN_01X12)
      (footprints
        (fp Pin_Header_Straight_1X40)
        (fp Pin_Header_Angled_1X40)
        (fp Socket_Strip_Straight_1X40)
        (fp Socket_Strip_Angled_1X40))
      (fields
        (field (name Reference) CON)
        (field (name Value) CONN_01X12))
      (pins
        (pin (num 0) (name P0) (type passive))
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))
        (pin (num 6) (name P6) (type passive))
        (pin (num 7) (name P7) (type passive))
        (pin (num 8) (name P8) (type passive))
        (pin (num 9) (name P9) (type passive))
        (pin (num 10) (name P10) (type passive))
        (pin (num 11) (name P11) (type passive))
        (pin (num 12) (name P12) (type passive))))
    (libpart (lib OLIMEX_Connectors) (part CONN_01X50)
      (footprints
        (fp Pin_Header_Straight_1X40)
        (fp Pin_Header_Angled_1X40)
        (fp Socket_Strip_Straight_1X40)
        (fp Socket_Strip_Angled_1X40))
      (fields
        (field (name Reference) CON)
        (field (name Value) CONN_01X50))
      (pins
        (pin (num 0) (name P0) (type passive))
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))
        (pin (num 6) (name P6) (type passive))
        (pin (num 7) (name P7) (type passive))
        (pin (num 8) (name P8) (type passive))
        (pin (num 9) (name P9) (type passive))
        (pin (num 10) (name P10) (type passive))
        (pin (num 11) (name P11) (type passive))
        (pin (num 12) (name P12) (type passive))
        (pin (num 13) (name P13) (type passive))
        (pin (num 14) (name P14) (type passive))
        (pin (num 15) (name P15) (type passive))
        (pin (num 16) (name P16) (type passive))
        (pin (num 17) (name P17) (type passive))
        (pin (num 18) (name P18) (type passive))
        (pin (num 19) (name P19) (type passive))
        (pin (num 20) (name P20) (type passive))
        (pin (num 21) (name P21) (type passive))
        (pin (num 22) (name P22) (type passive))
        (pin (num 23) (name P23) (type passive))
        (pin (num 24) (name P24) (type passive))
        (pin (num 25) (name P25) (type passive))
        (pin (num 26) (name P26) (type passive))
        (pin (num 27) (name P27) (type passive))
        (pin (num 28) (name P28) (type passive))
        (pin (num 29) (name P29) (type passive))
        (pin (num 30) (name P30) (type passive))
        (pin (num 31) (name P31) (type passive))
        (pin (num 32) (name P32) (type passive))
        (pin (num 33) (name P33) (type passive))
        (pin (num 34) (name P34) (type passive))
        (pin (num 35) (name P35) (type passive))
        (pin (num 36) (name P36) (type passive))
        (pin (num 37) (name P37) (type passive))
        (pin (num 38) (name P38) (type passive))
        (pin (num 39) (name P39) (type passive))
        (pin (num 40) (name P40) (type passive))
        (pin (num 41) (name P4) (type passive))
        (pin (num 42) (name P42) (type passive))
        (pin (num 43) (name P43) (type passive))
        (pin (num 44) (name P44) (type passive))
        (pin (num 45) (name P45) (type passive))
        (pin (num 46) (name P46) (type passive))
        (pin (num 47) (name P47) (type passive))
        (pin (num 48) (name P48) (type passive))
        (pin (num 49) (name P49) (type passive))
        (pin (num 50) (name P50) (type passive))))
    (libpart (lib OLIMEX_IC) (part "AR1021T-I_SS(SSOP-20)")
      (fields
        (field (name Reference) U)
        (field (name Value) "AR1021T-I_SS(SSOP-20)"))
      (pins
        (pin (num 1) (name VDD) (type power_in))
        (pin (num 2) (name M1) (type input))
        (pin (num 3) (name SY-) (type input))
        (pin (num 4) (name M2) (type input))
        (pin (num 5) (name WAKE) (type input))
        (pin (num 6) (name SIQ) (type output))
        (pin (num 7) (name SY+) (type input))
        (pin (num 8) (name SS) (type input))
        (pin (num 9) (name SDO/I2C_IRQ) (type output))
        (pin (num 10) (name NC) (type NotConnected))
        (pin (num 11) (name SCK/SCL/TX) (type BiDi))
        (pin (num 12) (name NC) (type NotConnected))
        (pin (num 13) (name SDI/SDA/RX) (type BiDi))
        (pin (num 14) (name SX+) (type input))
        (pin (num 15) (name Y+) (type output))
        (pin (num 16) (name Y-) (type output))
        (pin (num 17) (name 5WSX-) (type input))
        (pin (num 18) (name X+) (type output))
        (pin (num 19) (name X-) (type output))
        (pin (num 20) (name VSS) (type power_in))))
    (libpart (lib OLIMEX_IC) (part "NS2009(MSOP-10)")
      (description "4-Wire Touch Screen Controller with I2C Interface")
      (fields
        (field (name Reference) U)
        (field (name Value) "NS2009(MSOP-10)")
        (field (name Footprint) OLIMEX_IC-FP:MSOP-10_Pitch-0.5mm_3.00x3.00x1.00mm))
      (pins
        (pin (num 1) (name VDD) (type power_in))
        (pin (num 2) (name XP) (type input))
        (pin (num 3) (name YP) (type input))
        (pin (num 4) (name XN) (type input))
        (pin (num 5) (name YN) (type input))
        (pin (num 6) (name GND) (type power_in))
        (pin (num 7) (name PENIRQ) (type output))
        (pin (num 8) (name A0) (type input))
        (pin (num 9) (name SDA) (type BiDi))
        (pin (num 10) (name SCL) (type input))))
    (libpart (lib OLIMEX_Jumpers) (part SJ)
      (footprints
        (fp *SJ*)
        (fp *SJ-CLOSE*)
        (fp *SJ_1_SMALLER_CLOSE*)
        (fp *SJ_1_SMALLER_CLOSE_10MILS*)
        (fp *SJ_1_THE_SMALLEST*)
        (fp *SJ_1_SMALLER*)
        (fp *SJW*))
      (fields
        (field (name Reference) SJ)
        (field (name Value) SJ)
        (field (name Footprint) jumper_SJ))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib OLIMEX_Jumpers) (part "SJ2W_Closed(1-2)")
      (footprints
        (fp *SJ_2*)
        (fp *SJ_2_SMALL*)
        (fp *SJ_2_SMALLER*)
        (fp *SJ_2_SMALL_23_TIED*)
        (fp *SJ_2_SMALL_12_TIED*)
        (fp *SJ_2_SMALLER_12_TIED*)
        (fp *SJ_2_SMALLER_23_TIED*)
        (fp *SJ_2W*))
      (fields
        (field (name Reference) SJ)
        (field (name Value) "SJ2W_Closed(1-2)"))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num 3) (name 3) (type passive))))
    (libpart (lib OLIMEX_RCL) (part C_Small)
      (footprints
        (fp C?)
        (fp C_????_*)
        (fp C_????)
        (fp SMD*_c)
        (fp Capacitor*))
      (fields
        (field (name Reference) C)
        (field (name Value) C_Small))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib OLIMEX_RCL) (part R_Small)
      (footprints
        (fp Resistor_*)
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R_Small))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib OLIMEX_Transistors) (part P-MOS+DIOD)
      (fields
        (field (name Reference) FET)
        (field (name Value) P-MOS+DIOD))
      (pins
        (pin (num 1) (name ~) (type input))
        (pin (num 2) (name ~) (type passive))
        (pin (num 3) (name ~) (type passive)))))
  (libraries
    (library (logical OLIMEX_Connectors)
      (uri /home/penko/SVN_Checkout/KiCAD_Components/OLIMEX_Connectors.lib))
    (library (logical OLIMEX_IC)
      (uri /home/penko/SVN_Checkout/KiCAD_Components/OLIMEX_IC.lib))
    (library (logical OLIMEX_Jumpers)
      (uri /home/penko/SVN_Checkout/KiCAD_Components/OLIMEX_Jumpers.lib))
    (library (logical OLIMEX_RCL)
      (uri /home/penko/SVN_Checkout/KiCAD_Components/OLIMEX_RCL.lib))
    (library (logical OLIMEX_Transistors)
      (uri /home/penko/SVN_Checkout/KiCAD_Components/OLIMEX_Transistors.lib)))
  (nets
    (net (code 1) (name "Net-(LCD1-Pad36)")
      (node (ref LCD1) (pin 36)))
    (net (code 2) (name "Net-(LCD1-Pad37)")
      (node (ref LCD1) (pin 37)))
    (net (code 3) (name /TXD)
      (node (ref SJ4) (pin 3))
      (node (ref mUEXT1) (pin 4))
      (node (ref UEXT1) (pin 4))
      (node (ref SJ3) (pin 2)))
    (net (code 4) (name /RXD)
      (node (ref SJ2) (pin 3))
      (node (ref SJ5) (pin 3))
      (node (ref UEXT1) (pin 3))
      (node (ref mUEXT1) (pin 3)))
    (net (code 5) (name /SDA)
      (node (ref U2) (pin 9))
      (node (ref SJ5) (pin 1))
      (node (ref mUEXT1) (pin 6))
      (node (ref UEXT1) (pin 6)))
    (net (code 6) (name /SCL)
      (node (ref UEXT1) (pin 5))
      (node (ref SJ4) (pin 1))
      (node (ref mUEXT1) (pin 5))
      (node (ref U2) (pin 10)))
    (net (code 7) (name /MOSI)
      (node (ref UEXT1) (pin 8))
      (node (ref mUEXT1) (pin 8))
      (node (ref LCD1) (pin 12)))
    (net (code 8) (name GND)
      (node (ref C5) (pin 2))
      (node (ref R2) (pin 1))
      (node (ref R3) (pin 1))
      (node (ref R4) (pin 1))
      (node (ref C3) (pin 1))
      (node (ref C6) (pin 2))
      (node (ref C1) (pin 1))
      (node (ref U1) (pin 17))
      (node (ref U1) (pin 14))
      (node (ref U1) (pin 8))
      (node (ref U1) (pin 7))
      (node (ref U1) (pin 4))
      (node (ref U1) (pin 3))
      (node (ref U1) (pin 20))
      (node (ref C2) (pin 2))
      (node (ref mUEXT1) (pin 0))
      (node (ref LCD1) (pin 2))
      (node (ref LCD1) (pin 20))
      (node (ref UEXT1) (pin 2))
      (node (ref SJ2) (pin 1))
      (node (ref U2) (pin 8))
      (node (ref U2) (pin 6))
      (node (ref LCD1) (pin 21))
      (node (ref C4) (pin 2))
      (node (ref R1) (pin 1))
      (node (ref LCD1) (pin 19))
      (node (ref mUEXT1) (pin 11))
      (node (ref LCD1) (pin 34))
      (node (ref LCD1) (pin 33))
      (node (ref LCD1) (pin 32))
      (node (ref LCD1) (pin 31))
      (node (ref mUEXT1) (pin 12))
      (node (ref LCD1) (pin 30))
      (node (ref LCD1) (pin 29))
      (node (ref LCD1) (pin 28))
      (node (ref LCD1) (pin 0))
      (node (ref LCD1) (pin 1))
      (node (ref LCD1) (pin 17))
      (node (ref LCD1) (pin 18))
      (node (ref SJ1) (pin 1))
      (node (ref LCD1) (pin 6))
      (node (ref LCD1) (pin 9))
      (node (ref LCD1) (pin 45))
      (node (ref LCD1) (pin 7))
      (node (ref LCD1) (pin 4))
      (node (ref LCD1) (pin 26))
      (node (ref LCD1) (pin 8))
      (node (ref LCD1) (pin 25))
      (node (ref LCD1) (pin 24))
      (node (ref LCD1) (pin 23))
      (node (ref LCD1) (pin 22))
      (node (ref LCD1) (pin 27)))
    (net (code 9) (name +3V3)
      (node (ref R9) (pin 2))
      (node (ref C2) (pin 1))
      (node (ref LCD1) (pin 3))
      (node (ref LCD1) (pin 42))
      (node (ref C5) (pin 1))
      (node (ref R8) (pin 2))
      (node (ref LCD1) (pin 43))
      (node (ref LCD1) (pin 44))
      (node (ref C3) (pin 2))
      (node (ref LCD1) (pin 5))
      (node (ref U1) (pin 1))
      (node (ref mUEXT1) (pin 1))
      (node (ref C6) (pin 1))
      (node (ref FET1) (pin 2))
      (node (ref mUEXT1) (pin 2))
      (node (ref C1) (pin 2))
      (node (ref SJ1) (pin 3))
      (node (ref U2) (pin 1))
      (node (ref R5) (pin 1))
      (node (ref R10) (pin 1))
      (node (ref UEXT1) (pin 1)))
    (net (code 10) (name /D\C)
      (node (ref UEXT1) (pin 7))
      (node (ref LCD1) (pin 13))
      (node (ref mUEXT1) (pin 7)))
    (net (code 11) (name /SCK)
      (node (ref LCD1) (pin 10))
      (node (ref mUEXT1) (pin 9))
      (node (ref UEXT1) (pin 9)))
    (net (code 12) (name /CS)
      (node (ref UEXT1) (pin 10))
      (node (ref LCD1) (pin 15))
      (node (ref mUEXT1) (pin 10)))
    (net (code 13) (name "Net-(SJ1-Pad2)")
      (node (ref U1) (pin 2))
      (node (ref SJ1) (pin 2)))
    (net (code 14) (name "Net-(R6-Pad1)")
      (node (ref R6) (pin 1))
      (node (ref SJ2) (pin 2)))
    (net (code 15) (name "Net-(R8-Pad1)")
      (node (ref SJ4) (pin 2))
      (node (ref U1) (pin 11))
      (node (ref R8) (pin 1)))
    (net (code 17) (name /XL)
      (node (ref U1) (pin 19))
      (node (ref U2) (pin 4))
      (node (ref LCD1) (pin 39))
      (node (ref R7) (pin 2)))
    (net (code 18) (name /XR)
      (node (ref U1) (pin 18))
      (node (ref U2) (pin 2))
      (node (ref LCD1) (pin 41)))
    (net (code 19) (name /YD)
      (node (ref U2) (pin 5))
      (node (ref U1) (pin 16))
      (node (ref LCD1) (pin 40)))
    (net (code 20) (name /YU)
      (node (ref U1) (pin 15))
      (node (ref LCD1) (pin 38))
      (node (ref U2) (pin 3)))
    (net (code 22) (name /LEDK3)
      (node (ref R1) (pin 2))
      (node (ref LCD1) (pin 46)))
    (net (code 23) (name /LEDA)
      (node (ref LCD1) (pin 50))
      (node (ref FET1) (pin 3)))
    (net (code 24) (name "Net-(FET1-Pad1)")
      (node (ref FET1) (pin 1))
      (node (ref R6) (pin 2))
      (node (ref R5) (pin 2)))
    (net (code 25) (name /MISO)
      (node (ref LCD1) (pin 35)))
    (net (code 26) (name /LEDK2)
      (node (ref LCD1) (pin 47))
      (node (ref R2) (pin 2)))
    (net (code 27) (name /LEDK1)
      (node (ref R3) (pin 2))
      (node (ref LCD1) (pin 48)))
    (net (code 28) (name /LEDK0)
      (node (ref LCD1) (pin 49))
      (node (ref R4) (pin 2)))
    (net (code 29) (name /RESET)
      (node (ref R10) (pin 2))
      (node (ref LCD1) (pin 11))
      (node (ref C4) (pin 1)))
    (net (code 30) (name /NRD)
      (node (ref LCD1) (pin 14)))
    (net (code 31) (name /TE)
      (node (ref LCD1) (pin 16)))
    (net (code 32) (name "Net-(R7-Pad1)")
      (node (ref R7) (pin 1))
      (node (ref U1) (pin 5)))
    (net (code 33) (name "Net-(R9-Pad1)")
      (node (ref R9) (pin 1))
      (node (ref SJ5) (pin 2))
      (node (ref U1) (pin 13)))
    (net (code 34) (name "Net-(U1-Pad6)")
      (node (ref U1) (pin 6)))
    (net (code 35) (name /I2C-IRQ)
      (node (ref U1) (pin 9))
      (node (ref U2) (pin 7))
      (node (ref SJ3) (pin 1)))
    (net (code 36) (name "Net-(U1-Pad10)")
      (node (ref U1) (pin 10)))
    (net (code 37) (name "Net-(U1-Pad12)")
      (node (ref U1) (pin 12)))))